We have chosen to make 3 offers.

This because video detection from the outside camera can be complicated.
Standard video detection from camera provides alarms from clouds, sun lights from cars, leaves blowing, snow, rain .etc

Offer 1
Here we have chosen to use internal IR detectors in admin building, container and transformers, which gives full alarm to security company and security guard when illegal entry into the building.
You can also get a warning when moving outside on the cameras. The downside may be that you get alerts from light, clouds, leaves, birds, etc. (such are all simple systems with motion detections from camera)

Offers 2
We have chosen that 10 of the cameras around the containers / transformers will have professional video detection. So when someone is moving around the containers / transformers, there will be a full alarm to the security company.
(This is advanced technology, and requires hi competence people to program / deliver professional video detection.)

We have not chosen a professional video-detection around admin building, (only normal) but can of course deliver it here. By illegal entry into the admin building, full alarm will go to the security company. You can also get a warning on pc or mobil when moving outside on the cameras.

Offer 3
When it`s fogging tightly or snowy, it is not 100% sure that the 10 professional cameras can see motions. To be 100% safe, we also offer thermal camera, which covers the entire area around containers / transformer.
(so are all professional systems, based on motion from camera, it's like putting a hood over the camera when fogging or tightly snowy)
We therefore recommend thermal camera as addition. 
We have in all 3 offers and added 2 cameras in the middle of the area between containers. This in order to see what happens if someone breaks within the ring of the 8 camera around the containers.

You can have a view of the camera system/ program in Oslo. Or we can show more about it in Alvdal.

We have planned to use PTZ camera on the 16 cameras outside. This allows you to control the camera from the keyboard to zoom in on objects ++.
Camera will automatically return to preprogrammed image / location after use.
Customer /securty company can log on to a PC to manage the cameras. 
We intend to place the cameras on the corner on the roof side of the transducers.  The best would have been to have, 4 posts on the area , one in each corner with camera mounted.
We plan to keep the storage device / recorder in the admin building.
Customer should consider whether this should be moved to one of the containers, so there will be some conversion on cabling.
We have also given an offer for 5 card readers .
We have not included locks or wiring for the card reader.
We have not brought any lift, so if we need lift to mount a camera, this will be added .